List to ask the tas

Why does writing the 3.3 to 5 volt not work on the setup for diptrace

How to properly use the voltage converter (5-3.3 programmatically)

How to put the voltage converter into the schematic

how to do the isr properly

-refer to interrupt for adc from sample code project

are overlaps allowed

roast our design for pcb compatibility

current limiter properly

Duty cycle percentages table 3

Table 4 do we say SLC\* or I/O pin?????