**List to ask the tas**

Why does writing the 3.3 to 5 volt not work on the setup for diptrace

How to properly use the voltage converter (5-3.3 programmatically)

Implement own up down voltage converter. Use resistors to go down and schematic of up down to go up

how to do the isr properly

-refer to interrupt for adc from sample code project

are overlaps allowed

Yes, but try not to.

Remember to assign a net class to every wire.